AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor/Outdoor Single Loose-Tube Dielectric
Armored Optical Fiber LS0H Cables
Description
2-12 fibers indoor/outdoor single loose-tube dielectric armored
dry-core single-jacket FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
Single PBT jell-filled loose tube
Strength elements & armor
Served swellable glass yarn
Cable jacket material
Flame retardant LS0H UV-resistant
compound
Fibers color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
30xOD mm
Long term bend radius
15xOD mm
Operating temperature
-30 to +70C
Installation temperature
0 to +50C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Panel Ordering Information
FF: Fiber Type
Max. Load N
Cable OD
Weight
Description
Short
Long
Packaging
P/N
mm
Kg/Km
Term
Term
2-Fiber LS0H FO Indoor/Outdoor Dielectric
8.0
75.0
2000
1000
2000m Drum
24R FF AA002N-BK2N
Armored Single Loose-Tube SJ Cable
4-Fiber LS0H FO Indoor/Outdoor Dielectric
8.0
75.0
2000
1000
2000m Drum
24R FF AA004N-BK2N
Armored Single Loose-Tube SJ Cable
6-Fiber LS0H FO Indoor/Outdoor Dielectric
8.0
75.0
2000
1000
2000m Drum
24R FF AA006N-BK2N
Armored Single Loose-Tube SJ Cable
8-Fiber LS0H FO Indoor/Outdoor Dielectric
8.0
75.0
2000
1000
2000m Drum
24R FF AA008N-BK2N
Armored Single Loose-Tube SJ Cable
10-Fiber LS0H FO Indoor/Outdoor Dielectric
8.0
75.0
2000
1000
2000m Drum
24R FF AA010N-BK2N
Armored Single Loose-Tube SJ Cable
12-Fiber LS0H FO Indoor/Outdoor Dielectric
8.0
75.0
2000
1000
2000m Drum
24R FF AA012N-BK2N
Armored Single Loose-Tube SJ Cable
B.1.3.2