AT&T Cabling Systems
FiberLine
AT&T FiberLine
Outdoor Single Loose-Tube Steel Armored
Double-Jacket Optical Fiber Cables
Description
2-12 fibers outdoor single loose-tube steel armored
double-jacket dry-core FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
Single PBT jell-filled loose tube
Strength elements
Served swellable glass yarn
Inner jacket material
PE
Armor
Corrugated steel tape
Outer jacket material
UV-resistant PE
Fibers color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
30xOD mm
Long term bend radius
15xOD mm
Operating temperature
-30 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Ordering Information
FF: Fiber Type
Max. Load N
Cable OD
Weight
Description
Short
Long
Packaging
P/N
mm
Kg/Km
Term
Term
2-Fiber FO Outdoor Steel Armored
11.0
115
1000
500
2000m Drum
24D FF CN002N-BK2N
Single Loose-Tube DJ Cable
4-Fiber FO Outdoor Steel Armored
11.0
115
1000
500
2000m Drum
24D FF CN004N-BK2N
Single Loose-Tube DJ Cable
6-Fiber FO Outdoor Steel Armored
11.0
115
1000
500
2000m Drum
24D FF CN006N-BK2N
Single Loose-Tube DJ Cable
8-Fiber FO Outdoor Steel Armored
11.0
115
1000
500
2000m Drum
24D FF CN008N-BK2N
Single Loose-Tube DJ Cable
10-Fiber FO Outdoor Steel Armored
11.0
115
1000
500
2000m Drum
24D FF CN010N-BK2N
Single Loose-Tube DJ Cable
12-Fiber FO Outdoor Steel Armored
11.0
120
1000
500
2000m Drum
24D FF CN012N-BK2N
Single Loose-Tube DJ Cable
B.1.7.3