AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic LC Connectors
Description
Fiber Optic Connectors Type LC
Durability
0.2dB max. change after 1000 mating cycles
Temperature range
-20 to +60C
Typical Insertion loss
<0.3dB
Ferrule type
Ceramic
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• EU Directive 2011/65/EU (RoHS-2)
Notes:
a. Each product has a full-length P/N that can be used as ordering information.
b. Each connector has a single letter code that can be used to build fiber-optic cords and pigtails part-numbers.
c. The default colors are indicated in this page. Other options available.
d. Each bag contains one connector and three colored boots: 0.9mm, 2.0mm & 3.0mm.
Ordering Information - Connectors
Compatible
Body
Boot
Type
Formation
Code
Packaging
P/N
Fiber
Color
Color
LC/UPC Connector
Multimode
Single
Beige
White
P
1/Bag 120/Box
29CM1NV001P-BG61
LC/UPC Connector
Singlemode
Single
Blue
White
Q
1/Bag 120/Box
29CS1NV001Q-BL61
LC/APC Connector
Singlemode
Single
Green
White
R
1/Bag 120/Box
29CS1NV001R-GN61
LC/UPC Connector
Multimode
Double
Beige
White
P
1/Bag 120/Box
29CM1NV002P-BG61
LC/UPC Connector
Singlemode
Double
Blue
White
Q
1/Bag 120/Box
29CS1NV002Q-BL61
LC/APC Connector
Singlemode
Double
Green
White
R
1/Bag 120/Box
29CS1NV002R-GN61
Ordering Information - Clips
Type
Color
Packaging
P/N
Duplex Clip for LC/UPC Multimode Connector
Beige
120/Bag
531M1NV002H-BG6Y
Duplex Clip for LC/UPC Singlemode Connector
Blue
120/Bag
531S1NV001Q-BL6Y
Duplex Clip for LC/APC Singlemode Connector
Green
120/Bag
531S1NV001R-GN6Y
B.4.1.5