AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic FC/UPC Simplex Multimode Cords
Description
This page shows some of the available combinations of AT&T fiber-optic
Simplex Multimode Cords made with multimode fibers and terminated with
FC/UPC connectors.
Additional combinations can be selected using the information on page B.3
Fiber type
Select a multimode fiber from page B.6
Buffer type
900µ tight flame retardant LS0H coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
Default jacket colors
MM OM3: Turquoise
MM OM4: Purple
Ordering Information
FF: Fiber Type CC: Jacket Color
Length
Cable OD
Description
Packaging
P/N
m
mm
FC/UPC-FC/UPC Simplex Multimode Cord LS0H
1
3.0
1/Bag - 12/Box
28C FF EE010T-CC 61
FC/UPC-FC/UPC Simplex Multimode Cord LS0H
2
3.0
1/Bag - 12/Box
28C FF EE020T-CC 61
FC/UPC-FC/UPC Simplex Multimode Cord LS0H
3
3.0
1/Bag - 12/Box
28C FF EE030T-CC 61
FC/UPC-FC/UPC Simplex Multimode Cord LS0H
5
3.0
1/Bag - 12/Box
28C FF EE050T-CC 61
FC/UPC-FC/UPC Simplex Multimode Cord LS0H
10
3.0
1/Bag - 12/Box
28C FF EE100T-CC61
FC/UPC-ST/UPC Simplex Multimode Cord LS0H
1
3.0
1/Bag - 12/Box
28C FF EA010T-CC 61
FC/UPC-ST/UPC Simplex Multimode Cord LS0H
2
3.0
1/Bag - 12/Box
28C FF EA020T-CC 61
FC/UPC-ST/UPC Simplex Multimode Cord LS0H
3
3.0
1/Bag - 12/Box
28C FF EA030T-CC 61
FC/UPC-ST/UPC Simplex Multimode Cord LS0H
5
3.0
1/Bag - 12/Box
28C FF EA050T-CC 61
FC/UPC-ST/UPC Simplex Multimode Cord LS0H
10
3.0
1/Bag - 12/Box
28C FF EA100T-CC 61
FC/UPC-LC/UPC Simplex Multimode Cord LS0H
1
2.0
1/Bag - 12/Box
28C FF EP010T-CC 61
FC/UPC-LC/UPC Simplex Multimode Cord LS0H
2
2.0
1/Bag - 12/Box
28C FF EP020T-CC 61
FC/UPC-LC/UPC Simplex Multimode Cord LS0H
3
2.0
1/Bag - 12/Box
28C FF EP030T-CC 61
FC/UPC-LC/UPC Simplex Multimode Cord LS0H
5
2.0
1/Bag - 12/Box
28C FF EP050T-CC 61
FC/UPC-LC/UPC Simplex Multimode Cord LS0H
10
2.0
1/Bag - 12/Box
28C FF EP100T-CC 61
FC/UPC-LSH/UPC Simplex Multimode Cord LS0H
1
2.0
1/Bag - 12/Box
28C FF ED010T-CC 61
FC/UPC-LSH/UPC Simplex Multimode Cord LS0H
2
2.0
1/Bag - 12/Box
28C FF ED020T-CC 61
FC/UPC-LSH/UPC Simplex Multimode Cord LS0H
3
2.0
1/Bag - 12/Box
28C FF ED030T-CC 61
FC/UPC-LSH/UPC Simplex Multimode Cord LS0H
5
2.0
1/Bag - 12/Box
28C FF ED050T-CC 61
FC/UPC-LSH/UPC Simplex Multimode Cord LS0H
10
2.0
1/Bag - 12/Box
28C FF ED100T-CC 61
Examples
FC/UPC-FC/UPC Simplex Cord LS0H OM1 Orange
1
3.0
1/Bag - 12/Box
28CM1EE010T-OR61
FC/UPC-ST/UPC Simplex Cord LS0H OM3 Turquoise
5
3.0
1/Bag - 12/Box
28CM3EA050T-TQ61
FC/UPC-LSH/UPC Simplex Cord LS0H OM4 Purple
10
2.0
1/Bag - 12/Box
28CM4ED100T-PU61
B.3.1.3.1