AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 5e LAN Copper Connectivity
Shielded & Unshielded RJ45 Industrial Jacks
Description
8P8C shielded RJ45 punch-down IP67 industrial jacks
Frequency range
1-100 MHz
Compatible conductors
22-24 AWG Solid or stranded
Pin-pair assignment
T568A & T568B (Universal)
Contacts
50µ-Inch Gold plating
Shield (if present)
Corrosion-resistant metal case
Housing
High impact FR compound
Protective covers
FR UV-resistant heavy-duty plastic material
Standard & EU Directives Conformance
• 100MHz connectors according to IEC 60603-7-2&3
• 100MHz connectors according to EN 60603-7-2&3
• Category 5e PL/Channel according to ANSI/TIA-568-C.2
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
• IEC 60259 IP67
• UL 1863 Communications-Circuit Accessories Safety
Mechanical & Electrical Properties
Orientation
180º
Termination blocks
LSA-Plus IDC
Insertion/withdrawal
750 cycles
Cable re-termination
20 terminations
Operating temperature
-25 to +70C at 5-93% RH
(Non condensing)
Ampacity
1.5 A max. @ 35C.
Contact resistance
20 mOhm max.
DC resistance
0.1 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
500 MegaOhm min. @100 Vdc
Recommended punch-down tool
LSA-Plus
Ordering Information
Jack
Cover
Description
Form
Packaging
P/N
Color
Color
8P8C RJ45 Unshielded CAT5e PD IP67 Industrial Keystone Jack
White
Black
Straight
1/Bag
15A5EFV008A-BK61
8P8C RJ45 Shielded CAT5e PD IP67 Industrial Keystone Jack
Metal
Black
Straight
1/Bag
15C5EFV008A-BK61
E.3.2