AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor/Outdoor Tight-Buffer Dielectric Armored
Double-Jacket Optical Fiber LS0H Cables
Description
6-144 fibers indoor/outdoor tight-buffer dielectric armored
double-jacket FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
900µ tight flame retardant LS0H coating
Strength elements
Served swellable aramid and glass yarn
Sub-units jacket material
Flame retardant LS0H compound
Multi-unit water blocking Swellable tapes
Inner jacket material
Flame retardant LS0H compound
Dielectric armor
Swellable glass yarn
Outer jacket material
Flame retardant LS0H UV-resistant
compound
Fibers and sub-units
TIA-598-C
color code
Jacket color
Black (other color available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Ordering Information
FF: Fiber Type
Max. Load N
Fiber
Cable OD
Weight
Description
Packaging
P/N
Count
mm
Kg/Km
Short
Long
Term
Term
2-Fiber LS0H FO Indoor/Outdoor
2
9.5
100
2000
1000
2000m Drum
23R FF AA002S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
4-Fiber LS0H FO Indoor/Outdoor
4
11.0
120
2000
1000
2000m Drum
23R FF AA004S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
6-Fiber LS0H FO Indoor/Outdoor
6
11.0
120
2000
1000
2000m Drum
23R FF AA006S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
8-Fiber LS0H FO Indoor/Outdoor
8
11.5
130
2000
1000
2000m Drum
23R FF AA008S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
12-Fiber LS0H FO Indoor/Outdoor
12
12.5
145
2000
1000
2000m Drum
23R FF AA012S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
16-Fiber LS0H FO Indoor/Outdoor
16
13.0
160
2500
1200
2000m Drum
23R FF AA016S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
18-Fiber LS0H FO Indoor/Outdoor
18
13.5
170
2500
1200
2000m Drum
23R FF AA018S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
24-Fiber LS0H FO Indoor/Outdoor
24
14.5
185
2500
1200
2000m Drum
23R FF AA024S-BK2N
Dielectric Armored Dry-Core Tight-Buffer DJ Cable
Continued on page B.1.3.1a
B.1.3.1