AT&T Cabling Systems
CenterLine
AT&T CenterLine Category 5e Plug & Play
Unshielded RJ21 (Telco) to RJ45 Plug & Play Patch Panels
Description
24 or 48 port unshielded panels (used with RJ21/RJ21 25-Pair cords)
Frequency range
1-100 MHz
Panel front
4 or 8 modules of 6 RJ45 jacks
Panel back
4 or 8 RJ21 (Telco) sockets
Color
Black
Shield
None
Housing
High impact FR compound
Frame
Galvanized steel
Standard & EU Directives Conformance
• Category 5e connecting hardware acc. to ANSI/TIA-568-C.2
• UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Port contacts
50µ-Inch gold plating
Insertion/Extraction durability
750 cycles
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Contact resistance
20 mOhm max.
DC resistance
0.2 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
10 MegaOhm min. @500 Vdc
Ordering Information
Size
Description
Color
Modules
Units
Packaging
P/N
mm
24 port RJ21/RJ45 Unshielded CAT5e 19’’ Patch Panel
Black
4
1U
44.4x483
1/Box
13U5ENV024A-BK1U
48 port RJ21/RJ45 Unshielded CAT5e 19’’ Patch Panel
Black
8
2U
89.0x483
1/Box
13U5ENV048A-BK2U
C.4.1.1