AT&T Cabling Systems
FiberLine
AT&T FiberLine Outlets
Fiber Optic Surface Mount Boxes
Description
1-4 fiber 86x86mm fiber optic surface mount boxes
Connector type compatibility
SC and LC
Type
Wall mount
Splicing and distribution options
1-4 fiber splicing
or cable distribution
Connectors assembly
One or two SC simplex
or LC duplex couplers
Access method
Top and back
Standard & EU Directives Conformance
• Plastic parts: UL94 V-0 flame test
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction
High-impact flame retardant materials
Operating temperature
0 to +60C at 5-85% RH (non condensing)
Storage temperature
-20 to +60C
Color
White (other colors available)
Ordering Information
Fiber
Size
Description
Ports
Color
Packaging
P/N
Capacity
mm
Fiber Optic Surface Mount Box
2
1-4
86x86x15
White
1/Bag
53F8686002N-WT61
B.5.1