AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 3
U/UTP 100 Ohm Horizontal and Backbone Outdoor SJ LAN Cables
Description
4-900 pair U/UTP outdoor cables
Frequency range
1-16 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Water blocking
Petroleum jelly
Color code
Modified ANSI/ICEA S-80-576
Shield
None
Jacket
Heavy duty UV resistant PE
Jacket color
Black
Standard & EU Directives Conformance
• Category 3 cable according to IEC 61156-4
• Category 3 cable according to ANSI/TIA-568-C.2
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max
Dynamic bend radius
8xOD mm min
Static bend radius
4xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max
Capacitance
66 pF/m max. @ 1KHz
Voltage rating
75 Vdc max
Velocity of propagation (NVP)
69% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
6.5
42
500m Drum
11U03EN004N-BK2K
4-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
6.5
42
1000m Drum
11U03EN004N-BK2L
25-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
12.7
200
1000m Drum
11U03EN025N-BK2L
100-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
22.5
830
1000m Drum
11U03EN100N-BK2L
200-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
30
1150
500m Drum
11U03EN200N-BK2K
300-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
35
1700
500m Drum
11U03EN300N-BK2K
400-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
41
2200
500m Drum
11U03EN400N-BK2K
600-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
49
3250
500m Drum
11U03EN600N-BK2K
900-Pair 24 AWG U/UTP CAT3 Outdoor SJ Cable Black
60
4900
500m Drum
11U03EN900N-BK2K
E.1.1