AT&T Cabling Systems
CopperLine
AT&T CopperLine Outlets
French Style Faceplates
Description
1-2 port French Style faceplates
Jack compatibility
Shielded or unshielded RJ45
keystone jacks
Category compatibility
CAT5e CAT6 CAT6A
Mount type
Wall or ducts
Shuttered
Yes
Color
White (other colors available)
KSJ insertion method
Back loading
Standard & EU Directives Conformance
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties and Features
Material of construction
High-impact flame retardant
materials
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Storage temperature
-20 to +80C
Ordering Information
Size
Description
Color
Ports
Labeling
Packaging
P/N
mm
French Style Back Box
White
N/A
81x81x45
None
1/Bag
16F00NV000A-WT61
French Style Faceplate with 45x45mm Opening
White
N/A
80x80x15
None
1/Bag
16F00NV000B-WT61
French Style Single-Port Flat Full-Size Module
White
1
45x45
Station ID
1/Bag
16F00NV001A-WT61
French Style Double-Port Flat Full-Size Module
White
2
45x45
Station ID
1/Bag
16F00NV002A-WT61
French Style Single-Port Angled Full-Size Module
White
1
45x45
Station ID
1/Bag
16F00NV001B-WT61
French Style Double-Port Angled Full-Size Module
White
2
45x45
Station ID
1/Bag
16F00NV002B-WT61
French Style Single-Port Flat Half-Size Module
White
1
22.5x45
Station ID
1/Bag
16F00NV001C-WT61
French Style Single-Port Angled Half-Size Module
White
1
22.5x45
Station ID
1/Bag
16F00NV001D-WT61
French Style Blank Flat Half-Size Module
White
0
22.5x45
Station ID
1/Bag
16F00NV000E-WT61
A.11.1