AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor Tight-Buffer Optical Fiber LS0H Cables
Description
2-144 fibers indoor tight-buffer FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
900µ tight flame retardant LS0H
coating
Strength elements
Served aramid and glass yarn
Central strength member
Dielectric, in multi-unit cables only
Sub-units jacket material
Flame retardant LS0H compound
Cable jacket material
Flame retardant LS0H compound
Fibers and sub-units color code TIA-598-C
Jacket color
Per request
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Ordering Information - Single Unit Cables
FF: Fiber Type CC: Jacket Color
Cable
Max. Load N
Fiber
Weight
Description
OD
Packaging
P/N
Count
Kg/Km
Short Term
Short Term
mm
2-Fiber LS0H FO Indoor Tight-Buffer Cable
2
3.5
15
600
200
2000m Drum
23N FF HA002S-CC 2N
4-Fiber LS0H FO Indoor Tight-Buffer Cable
4
5.0
22
600
200
2000m Drum
23N FF HA004S-CC 2N
6-Fiber LS0H FO Indoor Tight-Buffer Cable
6
5.0
23
600
200
2000m Drum
23N FF HA006S-CC 2N
8-Fiber LS0H FO Indoor Tight-Buffer Cable
8
5.5
27
600
200
2000m Drum
23N FF HA008S-CC 2N
12-Fiber LS0H FO Indoor Tight-Buffer Cable
12
6.3
35
600
200
2000m Drum
23N FF HA012S-CC 2N
16-Fiber LS0H FO Indoor Tight-Buffer Cable
16
7.0
45
1500
500
2000m Drum
23N FF HA016S-CC 2N
18-Fiber LS0H FO Indoor Tight-Buffer Cable
18
7.5
51
1500
500
2000m Drum
23N FF HA018S-CC 2N
24-Fiber LS0H FO Indoor Tight-Buffer Cable
24
8.5
60
1500
500
2000m Drum
23N FF HA024S-CC 2N
Ordering Information - Multi-Unit Cables
FF: Fiber Type CC: Jacket Color
Fiber
Cable
Max. Load N
Subunit
Weight
Description
per
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Subunit
mm
Term
Term
18-Fiber LS0H FO Indoor Tight-Buffer Cable
6
3
12
125
1500
500
2000m Drum
23N FF HA018M-CC 2N
24-Fiber LS0H FO Indoor Tight-Buffer Cable
6
4
13
135
1500
500
2000m Drum
23N FF HA024M-CC 2N
36-Fiber LS0H FO Indoor Tight-Buffer Cable
6
6
16
210
1500
500
2000m Drum
23N FF HA036M-CC 2N
48-Fiber LS0H FO Indoor Tight-Buffer Cable
12
4
16
210
1500
500
2000m Drum
23N FF HA048M-CC 2N
60-Fiber LS0H FO Indoor Tight-Buffer Cable
12
5
17
230
1500
500
2000m Drum
23N FF HA060M-CC 2N
72-Fiber LS0H FO Indoor Tight-Buffer Cable
12
6
19
300
1500
500
2000m Drum
23N FF HA072M-CC 2N
96-Fiber LS0H FO Indoor Tight-Buffer Cable
12
8
22
390
1500
500
2000m Drum
23N FF HA096M-CC 2N
144-Fiber LS0H FO Indoor Tight-Buffer Cable
12
12
28
600
1500
500
2000m Drum
23N FF HA144M-CC 2N
B.1.1.2