AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 3
Unshielded & Shielded Keystone Jacks
Description
4-10 wire unshielded or shielded jacks
Frequency range
1-16 MHz
Compatible conductors
23-26 AWG Solid or stranded
Pin-pair assignment
T568A & T568B (Universal)
Contacts
Gold plating over nickel plated
metal
Shield
Corrosion resistant metal casing
Housing
High impact FR compound
Standard & EU Directives Conformance
• Connectors according to IEC 60603-7
• Category 3 connecting hardware according to
ANSI/TIA-568-C.2
• UL94 V-0 flame tests
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Orientation
90°
IDC contacts
Punch-down 110 or LSA-Plus
Insertion/Extraction durability
750 cycles Level A durability
Cable re-termination
20 terminations
Operating temperature
-20 to +60C at 5-95% RH
(non condensing)
Contact resistance
20 mOhm max.
DC resistance
0.1 Ohm max.
Voltage rating
75 Vdc max.
Insulation resistance
500 MegaOhm min. @500 Vdc
Ordering Information
Description
Color
Packaging
P/N
4P4C RJ11 Unshielded CAT3 Keystone Jack
White
1/Bag
100/Box
15A03NV004N-WT5C
4P4C RJ11 Shielded CAT3 Keystone Jack
White
1/Bag
100/Box
15C03NV004N-WT5C
6P4C RJ11 Unshielded CAT3 Keystone Jack
White
1/Bag
100/Box
15A03NV004A-WT5C
6P4C RJ11 Shielded CAT3 Keystone Jack
White
1/Bag
100/Box
15C03NV004A-WT5C
6P6C RJ12 Unshielded CAT3 Keystone Jack
White
1/Bag
100/Box
15A03NV006N-WT5C
6P6C RJ12 Shielded CAT3 Keystone Jack
White
1/Bag
100/Box
15C03NV006N-WT5C
8P8C RJ45 Unshielded CAT3 Keystone Jack
White
1/Bag
100/Box
15A03NV008N-WT5C
8P8C RJ45 Shielded CAT3 Keystone Jack
White
1/Bag
100/Box
15C03NV008N-WT5C
10P10C RJ50 Unshielded CAT3 Keystone Jack
White
1/Bag
100/Box
15A03NV010N-WT5C
10P10C RJ50 Shielded CAT3 Keystone Jack
White
1/Bag
100/Box
15C03NV010N-WT5C
A.1.2