AT&T Cabling Systems
FiberLine
AT&T FiberLine
Outdoor Multi Loose-Tube Short-Span ADSS Optical Fiber Cables
Description
2-288 fibers outdoor all-dielectric self-supporting (ADSS)
short-span multi loose-tube jelly-filled double-jacket FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking
Petroleum jelly
Inner jacket material
PE
Peripheral strength elements
Jelly filled aramid yarn
Outer jacket material
UV-resistant PE
Fibers and tubes color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
23xOD mm
Long term bend radius
12xOD mm
Operating temperature
-40 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Default fiber count per tube
Indicated (other options available)
Load conditions
NESC Medium
Span
122m max.
Installation sag
1%
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber FO Outdoor Loose-Tube ADSS
2000m
2
1
5
14.0
155
9500
5300
25A FF EN002S-BK2N
Short-Span Jelly-Filled Cable
Drum
4-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
1
5
14.0
155
9500
5300
25A FF EN004S-BK2N
Short-Span Jelly-Filled Cable
Drum
6-Fiber FO Outdoor Loose-Tube ADSS
2000m
6
1
5
14.0
155
9500
5300
25A FF EN006S-BK2N
Short-Span Jelly-Filled Cable
Drum
8-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
2
4
14.5
170
9500
5300
25A FF EN008S-BK2N
Short-Span Jelly-Filled Cable
Drum
12-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
3
3
14.5
170
9500
5300
25A FF EN012S-BK2N
Short-Span Jelly-Filled Cable
Drum
24-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
6
0
14.5
170
9500
5300
25A FF EN024S-BK2N
Short-Span Jelly-Filled Cable
Drum
36-Fiber FO Outdoor Loose-Tube ADSS
2000m
6
6
0
14.5
170
9500
5300
25A FF EN024S-BK2N
Short-Span Jelly-Filled Cable
Drum
48-Fiber FO Outdoor Loose-Tube ADSS
2000m
8
6
0
14.5
175
10000
5900
25A FF EN048S-BK2N
Short-Span Jelly-Filled Cable
Drum
72-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
6
0
14.5
180
10000
5900
25A FF EN072S-BK2N
Short-Span Jelly-Filled Cable
Drum
96-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
8
0
16.5
230
13000
7000
25A FF EN096S-BK2N
Short-Span Jelly-Filled Cable
Drum
144-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
12
0
20.0
355
16000
9400
25A FF EN144S-BK2N
Short-Span Jelly-Filled Cable
Drum
288-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
24
0
22.5
510
16000
9400
25A FF EN288S-BK2N
Short-Span Jelly-Filled Cable
Drum
B.1.6.5