AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MTP Assemblies
MTP-MTP Fiber Optic Trunk Assemblies
Description
MTP female to MTP female straight LS0H trunk assemblies
for plug & play panels
Fiber type
Select a fiber from page B.6.
Cable type
12-fiber or 24-fiber tight-buffer round
ruggedized cable
Cable jackets material
Flame retardant LS0H compound
Inner jacket diameter
3.0 mm (12-fiber) or 5.5 mm (24-fiber)
Outer jacket diameter
6.5 mm (12-fiber) or 9.0 mm (24-fiber)
Connector type 12-fiber
One MTP female both sides
Connector type 24-fiber
Two MTP female both sides
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Ordering Information
FF: Fiber Type CC: Jacket Color
Fiber
Length
Cable OD
Description
Polarity
Packaging
P/N
Count
m
mm
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
5
6.5
1/Bag
85S FF HA005P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
10
6.5
1/Bag
85S FF HA010P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
20
6.5
1/Bag
85S FF HA020P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
30
6.5
1/Bag
85S FF HA030P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
40
6.5
1/Bag
85S FF HA040P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
50
6.5
1/Bag
85S FF HA050P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
60
6.5
1/Bag
85S FF HA060P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
70
6.5
1/Bag
85S FF HA070P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
80
6.5
1/Bag
85S FF HA080P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
90
6.5
1/Bag
85S FF HA090P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
12
100
6.5
1/Bag
85S FF HA100P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
5
9.0
1/Bag
86S FF HA005P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
10
9.0
1/Bag
86S FF HA010P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
20
9.0
1/Bag
86S FF HA020P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
30
9.0
1/Bag
86S FF HA030P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
40
9.0
1/Bag
86S FF HA040P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
50
9.0
1/Bag
86S FF HA050P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
60
9.0
1/Bag
86S FF HA060P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
70
9.0
1/Bag
86S FF HA070P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
80
9.0
1/Bag
86S FF HA080P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
90
9.0
1/Bag
86S FF HA090P-CC 61
MTP Female - MTP Female Plug & Play LS0H Trunk Assembly
Straight
24
100
9.0
1/Bag
86S FF HA100P-CC 61
C.5.4.1.2