AT&T Cabling Systems
Outdoorline
AT&T Outdoorline
Outdoor Multi Loose-Tube Steel Armored
Jelly-Filled Single-Jacket Optical Fiber Cables
Description
2-288 fibers outdoor multi loose-tube jelly-filled single-jacket
steel-armored FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking
Petroleum jelly
Armor
Corrugated st
Cable jacket material
UV-resistant
Fibers and tubes color code
TIA-598-C
Jacket color
Black (other
Standard & EU Directives Conformanc
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-40 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m
24h - IEC 607
Default fiber count per tube
Indicated (other options available)
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber FO Outdoor Loose-Tube
2000m
2
1
5
11.7
135
2700
1700
25S FF CN002N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
4-Fiber FO Outdoor Loose-Tube
2000m
4
1
5
11.7
135
2700
1700
25S FF CN004N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
6-Fiber FO Outdoor Loose-Tube
2000m
6
1
5
11.7
135
2700
1700
25S FF CN006N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
8-Fiber FO Outdoor Loose-Tube
2000m
4
2
4
11.7
135
2700
1700
25S FF CN008N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
12-Fiber FO Outdoor Loose-Tube
2000m
4
3
3
11.7
135
2700
1700
25S FF CN012N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
24-Fiber FO Outdoor Loose-Tube
2000m
4
6
0
11.7
135
2700
1700
25S FF CN024N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
36-Fiber FO Outdoor Loose-Tube
2000m
6
6
0
11.7
135
2700
1700
25S FF CN036N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
48-Fiber FO Outdoor Loose-Tube
2000m
8
6
0
12.8
165
2700
1700
25S FF CN048N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
72-Fiber FO Outdoor Loose-Tube
2000m
12
6
0
13.5
185
2700
1700
25S FF CN072N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
96-Fiber FO Outdoor Loose-Tube
2000m
12
8
0
14.9
215
2700
1700
25S FF CN096N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
144-Fiber FO Outdoor Loose-Tube
2000m
12
12
0
18.9
330
2700
1700
25S FF CN144N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
288-Fiber FO Outdoor Loose-Tube
2000m
12
24
0
22.0
440
2700
1700
25S FF CN288N-BK2N
Steel Armored Jelly-Filled SJ Cable
Drum
E.4.9