AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MPO Assemblies
MPO-MTRJ Fiber Optic Harnesses
Description
MPO female to FC/UPC LS0H modular harnesses for plug & play panels
Fiber type
Select a fiber from page B.6.
Cable type
12-fiber tight-buffer round cable
Cable jacket material
Flame retardant LS0H compound
Cable jacket diameter
3.0 mm nom.
Connector types
One MPO female and twelve FC/UPC
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Ordering Information
FF: Fiber Type CC: Jacket Color
Fiber
Length
Cable OD
Description
MPO
MTRJ
Packaging
P/N
Count
m
mm
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
2
3.0
1/Bag
80T FF HA002T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
3
3.0
1/Bag
80T FF HA003T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
5
3.0
1/Bag
80T FF HA005T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
10
3.0
1/Bag
80T FF HA010T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
15
3.0
1/Bag
80T FF HA015T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
20
3.0
1/Bag
80T FF HA020T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
25
3.0
1/Bag
80T FF HA025T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
30
3.0
1/Bag
80T FF HA030T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
40
3.0
1/Bag
80T FF HA040T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
50
3.0
1/Bag
80T FF HA050T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
60
3.0
1/Bag
80T FF HA060T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
70
3.0
1/Bag
80T FF HA070T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
80
3.0
1/Bag
80T FF HA080T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
90
3.0
1/Bag
80T FF HA090T-CC 61
MPO Female to MTRJ Female Plug & Play LS0H Harness
1
6
12
100
3.0
1/Bag
80T FF HA100T-CC 61
C.5.5.6