AT&T Cabling Systems
Outdoorline
AT&T Outdoorline
Outdoor Multi Loose-Tube Long-Span ADSS Optical Fiber Cables
Description
2-288 fibers outdoor all-dielectric self-supporting (ADSS) long-span
multi loose-tube jelly-filled double-jacket FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking
Petroleum jelly
Inner jacket material
PE
Peripheral strength elements
Jelly-filled aramid yarn
Outer jacket material
UV-resistant PE
Fibers and tubes color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
23xOD mm
Long term bend radius
12xOD mm
Operating temperature
-40 to +70C
Installation temperature
-20 to +70C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Default fiber count per tube
Indicated (other options available)
Load conditions
NESC Medium
Span
250m max.
Installation sag
1%
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber FO Outdoor Loose-Tube ADSS
2000m
2
1
5
15.0
175
16000
9800
25A FF EN002L-BK2N
Long-Span Jelly-Filled Cable
Drum
4-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
1
5
15.0
175
16000
9800
25A FF EN004L-BK2N
Long-Span Jelly-Filled Cable
Drum
6-Fiber FO Outdoor Loose-Tube ADSS
2000m
6
1
5
15.0
175
16000
9800
25A FF EN006L-BK2N
Long-Span Jelly-Filled Cable
Drum
8-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
2
4
16.0
190
16000
9800
25A FF EN008L-BK2N
Long-Span Jelly-Filled Cable
Drum
12-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
3
3
16.0
200
16000
9800
25A FF EN012L-BK2N
Long-Span Jelly-Filled Cable
Drum
24-Fiber FO Outdoor Loose-Tube ADSS
2000m
4
6
0
16.0
205
16000
9800
25A FF EN024L-BK2N
Long-Span Jelly-Filled Cable
Drum
36-Fiber FO Outdoor Loose-Tube ADSS
2000m
6
6
0
16.0
210
16000
9800
25A FF EN036L-BK2N
Long-Span Jelly-Filled Cable
Drum
48-Fiber FO Outdoor Loose-Tube ADSS
2000m
8
6
0
16.0
215
18000
11000
25A FF EN048L-BK2N
Long-Span Jelly-Filled Cable
Drum
72-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
6
0
16.0
220
18000
11000
25A FF EN072L-BK2N
Long-Span Jelly-Filled Cable
Drum
96-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
8
0
21.0
360
21000
12900
25A FF EN096L-BK2N
Long-Span Jelly-Filled Cable
Drum
144-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
12
0
21.5
425
29000
29000
25A FF EN144L-BK2N
Long-Span Jelly-Filled Cable
Drum
288-Fiber FO Outdoor Loose-Tube ADSS
2000m
12
24
0
24.2
605
29000
29000
25A FF EN288L-BK2N
Long-Span Jelly-Filled Cable
Drum
E.4.7