AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic Connectors and Couplers
Description
This section shows all the available AT&T fiber-optic connectors and couplers.
Notes:
a. Each connector has a full-length P/N that can be used as ordering information for the connector alone.
b. Each connector has a single letter code that can be used to build fiber-optic cords and pigtails part-numbers.
c. The default boot colors are indicated in the following pages. Other options available.
Connector Type
Compatible Fiber
Code
ST/UPC
Multimode
A
ST/UPC
Singlemode
C
FC/UPC
Multimode
E
FC/UPC
Singlemode
F
FC/APC
Singlemode
G
SC/UPC
Multimode
H
SC/UPC
Singlemode
J
SC/APC
Singlemode
K
LSH/UPC
Multimode
D
LSH/UPC
Singlemode
L
LSH/APC
Singlemode
M
LC/UPC
Multimode
P
LC/UPC
Singlemode
Q
LC/APC
Singlemode
R
MTRJ Male
All fibers
S
MTRJ Female
All fibers
T
B.4.1