AT&T Cabling Systems
CenterLine
AT&T CenterLine Category 5e
Shielded 100 Ohm RJ45 Plug & Play Pre-Terminated Cassettes
Description
6-Port shielded RJ45 F/UTP pre-terminated cassettes in 24-Port panel
Frequency range
1-100 MHz
Cassette contents
6 shielded CAT5e RJ45 jacks
Panel formation
4 cassettes in 1U
Panel and cassette color
Black (other colors available)
Cable bundles
Conductor
24 AWG solid bare copper
Insulation
PO
Shield
Overall aluminum foil
Drain wire
Single tin-coated copper solid wire
Jacket
LS0H
Standard jacket color
Gray (other colors available)
Number of 4-pair cables
6 in each cassette
Bundle jacket
LS0H black polyester braid secured
with shrink-tubes
Length
5-50m (other lengths available)
Standard & EU Directives Conformance
• Category 5e according to ISO/IEC 11801
• Category 5e according to EN 50173
• Category 5e according to ANSI/TIA-568-C.2
• IEC 60332-1 (cable) and UL94 V-0 flame tests
(construction materials)
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Impedance
100 Ohm nom.
Pin-pair assignment
T568B
Jacks contacts
50µ-Inch Gold plating
Jacks housing
High impact FR compound
Jack shield
Die-cast metal case
Operating temperature
-20 to +60C
Voltage rating
75 Vdc max.
Ampacity
1.0 Ampere max.
Insulation resistance
500 MegaOhm min. @500 Vdc
Ordering Information
Bundle Length
Remote
Description
Packaging
P/N
m
Termination
24-Port Shielded Blank 19" Panel for 4 Pre-Terminated Cassettes
N/A
N/A
1/Box
13S00NV024P-BK51
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Cassette
10
RJ45 Cassette
1/Bag
32S5EHA100C-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Cassette
20
RJ45 Cassette
1/Bag
32S5EHA200C-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Cassette
30
RJ45 Cassette
1/Bag
32S5EHA300C-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Cassette
40
RJ45 Cassette
1/Bag
32S5EHA400C-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Cassette
50
RJ45 Cassette
1/Bag
32S5EHA500C-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Jacks
10
6 RJ45 Jack
1/Bag
32S5EHA100R-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Jacks
20
6 RJ45 Jack
1/Bag
32S5EHA200R-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Jacks
30
6 RJ45 Jack
1/Bag
32S5EHA300R-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Jacks
40
6 RJ45 Jack
1/Bag
32S5EHA400R-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Jacks
50
6 RJ45 Jack
1/Bag
32S5EHA500R-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Plugs
5
6 RJ45 Plugs
1/Bag
32S5EHA050L-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Plugs
10
6 RJ45 Plugs
1/Bag
32S5EHA100L-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Plugs
15
6 RJ45 Plugs
1/Bag
32S5EHA150L-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Plugs
20
6 RJ45 Plugs
1/Bag
32S5EHA200L-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Plugs
25
6 RJ45 Plugs
1/Bag
32S5EHA250L-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Open
10
None
1/Bag
32S5EHA100E-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Open
20
None
1/Bag
32S5EHA200E-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Open
30
None
1/Bag
32S5EHA300E-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Open
40
None
1/Bag
32S5EHA400E-BK61
6-Port Shielded CAT5e Plug & Play RJ45 Cassette to Open
50
None
1/Bag
32S5EHA500E-BK61
C.4.1.4