AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MPO Plug & Play
High-Density MPO Cassette Fiber Optic Panel (contd.)
Ordering Information - Cassettes
Front
Coupler
MPO
Size
Description
Polarity
Packaging
P/N
Couplers
Capacity
Ports
mm
Pre-loaded High-Density MPO Cassette
LC/UPC OM1
12
1
Straight
34x111x88
1/Box
82RM1HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM1
12
1
Flipped
34x111x88
1/Box
82DM1HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM1
24
2
Straight
34x111x88
1/Box
82RM1HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM1
24
2
Flipped
34x111x88
1/Box
82DM1HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM2
12
1
Straight
34x111x88
1/Box
82RM2HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM2
12
1
Flipped
34x111x88
1/Box
82DM2HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM2
24
2
Straight
34x111x88
1/Box
82RM2HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM2
24
2
Flipped
34x111x88
1/Box
82DM2HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3
12
1
Straight
34x111x88
1/Box
82RM3HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3
12
1
Flipped
34x111x88
1/Box
82DM3HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3
24
2
Straight
34x111x88
1/Box
82RM3HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3
24
2
Flipped
34x111x88
1/Box
82DM3HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3 BI
12
1
Straight
34x111x88
1/Box
82RC3HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3 BI
12
1
Flipped
34x111x88
1/Box
82DC3HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3 BI
24
2
Straight
34x111x88
1/Box
82RC3HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM3 BI
24
2
Flipped
34x111x88
1/Box
82DC3HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4
12
1
Straight
34x111x88
1/Box
82RM4HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4
12
1
Flipped
34x111x88
1/Box
82DM4HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4
24
2
Straight
34x111x88
1/Box
82RM4HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4
24
2
Flipped
34x111x88
1/Box
82DM4HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4 BI
12
1
Straight
34x111x88
1/Box
82RC4HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4 BI
12
1
Flipped
34x111x88
1/Box
82DC4HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4 BI
24
2
Straight
34x111x88
1/Box
82RC4HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OM4 BI
24
2
Flipped
34x111x88
1/Box
82DC4HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2
12
1
Straight
34x111x88
1/Box
82RS2HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2
12
1
Flipped
34x111x88
1/Box
82DS2HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2
24
2
Straight
34x111x88
1/Box
82RS2HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2
24
2
Flipped
34x111x88
1/Box
82DS2HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2 BI
12
1
Straight
34x111x88
1/Box
82RB2HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2 BI
12
1
Flipped
34x111x88
1/Box
82DB2HV012P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2 BI
24
2
Straight
34x111x88
1/Box
82RB2HV024P-BK51
Pre-loaded High-Density MPO Cassette
LC/UPC OS2 BI
24
2
Flipped
34x111x88
1/Box
82DB2HV024P-BK51
Blank High-Density Cassette
None
N/A
N/A
N/A
34x111x88
1/Box
82K00NV000N-BK51
BI = Bend-Insensitive
C.5.2.2a