AT&T Cabling Systems
OutdoorLine
AT&T OutdoorLine
Outdoor Fiber-optic Splice Closures (contd.)
Ordering Information
Size mm
Cable Ports
FO
Total
Splicing
Single
Max.
Description
Cable
Fiber
Tray
Tray
Packaging
P/N
Amount
Cable
Height
Diameter
Type
Capacity
Type
Capacity
& Type
Diameter
mm
Outdoor Fiber-optic
4 Round
20.0
Dome Splice Closure
495
220
Ribbon
288
D0
72
1/Box
53S00KNG0D4-BK51
Type G0D4
1 Oval
35.0
Outdoor Fiber-optic
4 Round
20.0
Dome Splice Closure
495
220
Ribbon
1080
C0
216
1/Box
53S00KNG0D5-BK51
Type G0D5
1 Oval
35.0
Outdoor Fiber-optic
3 Round
21.0
Dome Splice Closure
530
205
Round
96
CH
12
1/Box
53S00KNGAA1-BK51
Type GAA1
1 Oval
30.0
Outdoor Fiber-optic
3 Round
21.0
Dome Splice Closure
530
205
Round
144
CI
24
1/Box
53S00KNGAA2-BK51
Type GAA2
1 Oval
30.0
Outdoor Fiber-optic
3 Round
21.0
Dome Splice Closure
530
205
Ribbon
432
D0
72
1/Box
53S00KNGAA3-BK51
Type GAA3
1 Oval
30.0
Outdoor Fiber-optic
2 Round
21.0
Dome Splice Closure
510
250
Round
192
CA
12
1/Box
53S00KNGAB1-BK51
Type GAB1
2 Oval
41.0
Outdoor Fiber-optic
2 Round
21.0
Dome Splice Closure
510
250
Round
382
BG
48
1/Box
53S00KNGAB2-BK51
Type GAB2
2 Oval
41.0
Outdoor Fiber-optic
2 Round
21.0
Dome Splice Closure
510
250
Round
720
BI
72
1/Box
53S00KNGAB3-BK51
Type GAB3
2 Oval
41.0
Outdoor Fiber-optic
2 Round
21.0
Dome Splice Closure
510
250
Ribbon
504
D0
72
1/Box
53S00KNGAB4-BK51
Type GAB4
2 Oval
41.0
Outdoor Fiber-optic
2 Round
21.0
Dome Splice Closure
510
250
Ribbon
1728
C0
216
1/Box
53S00KNGAB5-BK51
Type GAB5
2 Oval
41.0
E.5.1a