AT&T Cabling Systems
CenterLine
AT&T CenterLine
DC Enhanced Metered Power Distribution Units (PDU) (contd.)
Ordering Information - PDU
Branch
C13
C19
Dimensions
Description
Circuit
Metering
P/N
Sockets
Sockets
mm
Breakers
Individual
32A Zero U Enhanced Metered PDU
18
6
2x16A
62x56x1830
& Branch
612032A024A-BK51
& Overall
Ordering Information - Hot Plug Module
RJ11
Dry
Description
P/N
Ports
Contacts
Hot Plug Sensor Module
3
4
6100304HPSM-NS51
Ordering Information - Sensors & Detectors
Connection
Cable Length
Mounting
Description
P/N
Type
m
Method
Temperature Sensor
RJ11
3
Magnetic or Screws
610TMPS003A-NS51
Temperature + Humidity Sensor
RJ11
3
Magnetic or Screws
610TMHS003A-NS51
Airflow Sensor
RJ11
3
Magnetic or Screws
610ARFS003A-NS51
Smoke Detector
Dry Contact
N/A
Magnetic or Screws
610SMDT000A-NS51
Motion Detector
Dry Contact
N/A
Magnetic or Screws
610MODT000A-NS51
Door Status Detector
Dry Contact
N/A
Magnetic or Screws
610DODT000A-NS51
C.2.2a