AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic LC/UPC Duplex Multimode Zip-Cords
Description
This page shows some of the available combinations of AT&T fiber-optic
Duplex Multimode Zip-Cords made with multimode fibers and terminated
with LC/UPC connectors.
Additional combinations can be selected using the information on page B.3
Fiber type
Select a multimode fiber from page B.6
Buffer type
900µ tight flame retardant LS0H coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
Default jacket colors
MM OM3: Turquoise
MM OM4: Purple
Ordering Information
FF: Fiber Type CC: Jacket Color
Length
Cable OD
Description
Packaging
P/N
m
mm
LC/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
1
2.0x4.0
1/Bag - 12/Box
28D FF PP010T-CC 61
LC/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
2
2.0x4.0
1/Bag - 12/Box
28D FF PP020T-CC 61
LC/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
3
2.0x4.0
1/Bag - 12/Box
28D FF PP030T-CC 61
LC/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
5
2.0x4.0
1/Bag - 12/Box
28D FF PP050T-CC 61
LC/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
10
2.0x4.0
1/Bag - 12/Box
28D FF PP100T-CC 61
LC/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
1
2.0x4.0
1/Bag - 12/Box
28D FF PA010T-CC 61
LC/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
2
2.0x4.0
1/Bag - 12/Box
28D FF PA020T-CC 61
LC/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
3
2.0x4.0
1/Bag - 12/Box
28D FF PA030T-CC 61
LC/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
5
2.0x4.0
1/Bag - 12/Box
28D FF PA050T-CC 61
LC/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
10
2.0x4.0
1/Bag - 12/Box
28D FF PA100T-CC 61
LC/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
1
2.0x4.0
1/Bag - 12/Box
28D FF PE010T-CC 61
LC/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
2
2.0x4.0
1/Bag - 12/Box
28D FF PE020T-CC 61
LC/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
3
2.0x4.0
1/Bag - 12/Box
28D FF PE030T-CC 61
LC/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
5
2.0x4.0
1/Bag - 12/Box
28D FF PE050T-CC 61
LC/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
10
2.0x4.0
1/Bag - 12/Box
28D FF PE100T-CC 61
LC/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
1
2.0x4.0
1/Bag - 12/Box
28D FF PD010T-CC 61
LC/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
2
2.0x4.0
1/Bag - 12/Box
28D FF PD020T-CC 61
LC/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
3
2.0x4.0
1/Bag - 12/Box
28D FF PD030T-CC 61
LC/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
5
2.0x4.0
1/Bag - 12/Box
28D FF PD050T-CC 61
LC/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
10
2.0x4.0
1/Bag - 12/Box
28D FF PD100T-CC 61
LC/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF PT010T-CC 61
LC/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF PT020T-CC 61
LC/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF PT030T-CC 61
LC/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF PT050T-CC 61
LC/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF PT100T-CC 61
Examples
LC/UPC-LC/UPC Duplex Zip-Cord LS0H OM1 Orange
1
2.0x4.0
1/Bag - 12/Box
28DM1PP010T-OR61
LC/UPC-FC/UPC Duplex Zip-Cord LS0H OM3 Turquoise
5
2.0x4.0
1/Bag - 12/Box
28DM3PE050T-TQ61
LC/UPC-LSH/UPC Duplex Zip-Cord LS0H OM4 Purple
10
2.0x4.0
1/Bag - 12/Box
28DM4PD100T-PU61
B.3.2.2.1