AT&T Cabling Systems
CopperLine
AT&T CopperLine Category 5
F/UTP 100 Ohm Horizontal & Backbone Indoor LAN Cables
Description
4-100 pair F/UTP cables
Frequency range
1-100 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Color code
Modified ANSI/ICEA S-80-576
Shield
Overall aluminum foil
Drain wire
Single tin-coated copper solid
wire
Jacket
PVC or LS0H
Standard & EU Directives Conformance
• Category 5 cable according to ANSI/TIA-568-A
• IEC 60332-1, IEC 60332-3-24 or IEC 60332-3-25 flame tests
• IEC 60754 & IEC 61034 (LS0H cables)
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm 2 max.
Short term bend radius
8xOD mm
Long term bend radius
4xOD mm
Operating temperature
-20 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max.
Capacitance
56 pF/m max. @ 1KHz
Voltage rating
75 Vdc max.
Velocity of propagation (NVP)
69% nom.
Ordering Information
OD
Weight
Description
Packaging
P/N
mm
Kg/Km
4-Pair 24 AWG F/UTP CAT5 PVC IEC 60332-1 Cable Gray
5.0
34
500m Drum
11P05VA004N-GY2K
4-Pair 24 AWG F/UTP CAT5 LS0H IEC 60332-1 Cable Gray
5.0
34
500m Drum
11P05HA004N-GY2K
4-Pair 24 AWG F/UTP CAT5 PVC IEC 60332-1 Cable Gray
5.0
34
1000m Drum
11P05VA004N-GY2L
4-Pair 24 AWG F/UTP CAT5 LS0H IEC 60332-1 Cable Gray
5.0
34
1000m Drum
11P05HA004N-GY2L
25-Pair 24 AWG F/UTP CAT5 PVC IEC 60332-1 Cable Gray
12.8
185
500m Drum
11P05VA025N-GY2K
25-Pair 24 AWG F/UTP CAT5 LS0H IEC 60332-1 Cable Gray
12.8
185
500m Drum
11P05HA025N-GY2K
50-Pair 24 AWG F/UTP CAT5 PVC IEC 60332-1 Cable Gray
16.8
276
500m Drum
11P05VA050N-GY2K
50-Pair 24 AWG F/UTP CAT5 LS0H IEC 60332-1 Cable Gray
16.8
276
500m Drum
11P05HA050N-GY2K
100-Pair 24 AWG F/UTP CAT5 PVC IEC 60332-1 Cable Gray
30.5
677
500m Drum
11P05VA100N-GY2K
100-Pair 24 AWG F/UTP CAT5 LS0H IEC 60332-1 Cable Gray
30.5
677
500m Drum
11P05HA100N-GY2K
A.2.1.2