AT&T Cabling Systems
Outdoorline
AT&T Outdoorline Category 3
F/UTP 100 Ohm Horizontal and Backbone Outdoor DJ CSA LAN Cables
Description
4-900 pair F/UTP shielded outdoor double-jacketed cables with
corrugated steel tape armor
Frequency range
1-16 MHz
Conductor
24 AWG Solid bare copper
Insulation
PO
Longitudinal water blocking Petroleum jelly
Color code
Modified ANSI/ICEA S-80-576
Shield
Overall aluminum foil
Drain wire
Solid tin-coated copper wire
Inner jacket
Heavy duty UV resistant PE
Armor and radial water
150µ Corrugated steel tape armor (CSA)
blocking
Outer jacket
UV resistant MDPE for outdoor use
Jacket color
Black
Standard & EU Directives Conformance
• Category 3 cable according to IEC 61156-4
• Category 3 cable according to ANSI/TIA-568-C.2
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Pulling force
50 N/mm2 max
Dynamic bend radius
50xOD mm min
Static bend radius
25xOD mm min
Operating temperature
-25 to +60C
Installation temperature
0 to +50C
DC resistance
93 Ohm/Km max
Capacitance
66 pF/m max. @ 1KHz
Voltage rating
75 Vdc max
Velocity of propagation (NVP)
69% nom.
Ordering Information
Inner OD
Jacket
OD
Weight
Description
Packaging
P/N
mm
Type
mm
Kg/Km
4-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
8.0
CSA+PE
13.5
107
500m Drum
11P03CN004N-BK2K
4-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
8.0
CSA+PE
13.5
107
1000m Drum
11P03CN004N-BK2L
25-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
12.6
CSA+PE
18
288
1000m Drum
11P03CN025N-BK2L
100-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
21.5
CSA+PE
27
780
1000m Drum
11P03CN100N-BK2L
200-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
29
CSA+PE
34.5
1660
500m Drum
11P03CN200N-BK2K
300-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
35
CSA+PE
40
2320
500m Drum
11P03CN300N-BK2K
400-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
39
CSA+PE
44
2920
500m Drum
11P03CN400N-BK2K
600-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
48
CSA+PE
53
4260
500m Drum
11P03CN600N-BK2K
900-Pair 24 AWG F/UTP CAT3 Outdoor CSA Cable Black
57
CSA+PE
62
6080
500m Drum
11P03CN900N-BK2K
E.1.6