AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MTP Plug & Play
High-Density MTP Cassette Fiber Optic Panel (contd.)
Ordering Information - Cassettes
Front
Coupler
MTP
Size
Description
Polarity
Packaging
P/N
Couplers
Capacity
Ports
mm
Pre-loaded High-Density MTP Cassette
LC/UPC OM1
12
1
Straight
34x111x88
1/Box
82GM1HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM1
12
1
Flipped
34x111x88
1/Box
82PM1HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM1
24
2
Straight
34x111x88
1/Box
82GM1HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM1
24
2
Flipped
34x111x88
1/Box
82PM1HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM2
12
1
Straight
34x111x88
1/Box
82GM2HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM2
12
1
Flipped
34x111x88
1/Box
82PM2HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM2
24
2
Straight
34x111x88
1/Box
82GM2HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM2
24
2
Flipped
34x111x88
1/Box
82PM2HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3
12
1
Straight
34x111x88
1/Box
82GM3HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3
12
1
Flipped
34x111x88
1/Box
82PM3HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3
24
2
Straight
34x111x88
1/Box
82GM3HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3
24
2
Flipped
34x111x88
1/Box
82PM3HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3 BI
12
1
Straight
34x111x88
1/Box
82GC3HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3 BI
12
1
Flipped
34x111x88
1/Box
82PC3HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3 BI
24
2
Straight
34x111x88
1/Box
82GC3HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM3 BI
24
2
Flipped
34x111x88
1/Box
82PC3HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4
12
1
Straight
34x111x88
1/Box
82GM4HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4
12
1
Flipped
34x111x88
1/Box
82PM4HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4
24
2
Straight
34x111x88
1/Box
82GM4HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4
24
2
Flipped
34x111x88
1/Box
82PM4HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4 BI
12
1
Straight
34x111x88
1/Box
82GC4HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4 BI
12
1
Flipped
34x111x88
1/Box
82PC4HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4 BI
24
2
Straight
34x111x88
1/Box
82GC4HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OM4 BI
24
2
Flipped
34x111x88
1/Box
82PC4HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2
12
1
Straight
34x111x88
1/Box
82GS2HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2
12
1
Flipped
34x111x88
1/Box
82PS2HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2
24
2
Straight
34x111x88
1/Box
82GS2HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2
24
2
Flipped
34x111x88
1/Box
82PS2HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2 BI
12
1
Straight
34x111x88
1/Box
82GB2HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2 BI
12
1
Flipped
34x111x88
1/Box
82PB2HV012P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2 BI
24
2
Straight
34x111x88
1/Box
82GB2HV024P-BK51
Pre-loaded High-Density MTP Cassette
LC/UPC OS2 BI
24
2
Flipped
34x111x88
1/Box
82PB2HV024P-BK51
Blank High-Density Cassette
None
N/A
N/A
N/A
34x111x88
1/Box
82K00NV000N-BK51
BI = Bend-Insensitive
C.5.1.2a