AT&T Cabling Systems
CenterLine
AT&T CenterLine Category 6A
Unshielded 100 Ohm RJ45 Plug & Play Pre-Terminated Cassettes
Description
6-Port unshielded RJ45 pre-terminated cassettes in 24-Port panel
Frequency range
1-500 MHz
Cassette contents
6 unshielded CAT6A RJ45 jacks
Panel formation
4 cassettes in 1U
Panel and cassette color
Black (other colors available)
Cable bundles
Conductor
23 AWG solid bare copper
Insulation
PO
Jacket
LS0H
Standard jacket color
Gray (other colors available)
Number of 4-pair cables
6 in each cassette
Bundle jacket
LS0H black polyester braid
secured with shrink-tubes
Length
5-50m (other lengths available)
Standard & EU Directives Conformance
• Category 6A according to ISO/IEC 11801
• Category 6A according to EN 50173
• Category 6A according to ANSI/TIA-568-C.2
• IEC 60332-1 (cable) and UL94 V-0 flame tests
(construction materials)
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical & Electrical Properties
Impedance
100 Ohm nom.
Pin-pair assignment
T568B
Jacks contacts
50µ-Inch Gold plating
Jacks housing
High impact FR compound
Operating temperature
-20 to +60C
Voltage rating
75 Vdc max.
Ampacity
1.0 Ampere max.
Insulation resistance
500 MegaOhm min. @500 Vdc
Ordering Information
Bundle Length
Remote
Description
Packaging
P/N
m
Termination
24-Port Unshielded Blank 19" Panel for 4 Pre-Terminated Cassettes
N/A
N/A
1/Box
13U00NV024P-BK51
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Cassette
10
RJ45 Cassette
1/Bag
32U6AHA100C-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Cassette
20
RJ45 Cassette
1/Bag
32U6AHA200C-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Cassette
30
RJ45 Cassette
1/Bag
32U6AHA300C-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Cassette
40
RJ45 Cassette
1/Bag
32U6AHA400C-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Cassette
50
RJ45 Cassette
1/Bag
32U6AHA500C-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Jacks
10
6 RJ45 Jack
1/Bag
32U6AHA100R-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Jacks
20
6 RJ45 Jack
1/Bag
32U6AHA200R-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Jacks
30
6 RJ45 Jack
1/Bag
32U6AHA300R-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Jacks
40
6 RJ45 Jack
1/Bag
32U6AHA400R-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Jacks
50
6 RJ45 Jack
1/Bag
32U6AHA500R-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Plugs
5
6 RJ45 Plugs
1/Bag
32U6AHA050L-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Plugs
10
6 RJ45 Plugs
1/Bag
32U6AHA100L-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Plugs
15
6 RJ45 Plugs
1/Bag
32U6AHA150L-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Plugs
20
6 RJ45 Plugs
1/Bag
32U6AHA200L-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Plugs
25
6 RJ45 Plugs
1/Bag
32U6AHA250L-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Open
10
None
1/Bag
32U6AHA100E-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Open
20
None
1/Bag
32U6AHA200E-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Open
30
None
1/Bag
32U6AHA300E-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Open
40
None
1/Bag
32U6AHA400E-BK61
6-Port Unshielded CAT6A Plug & Play RJ45 Cassette to Open
50
None
1/Bag
32U6AHA500E-BK61
C.4.3.1