AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MPO Assemblies
MPO-MPO Fiber Optic Cords
Description
MPO female to MPO female straight LS0H modular cords
for plug & play panels
Fiber type
Select a fiber from page B.6.
Cable type
12-fiber ribbon cable
Cable jacket material
Flame retardant LS0H compound
Cable jacket dimensions
5.0x2.5 mm nom.
Connector type
MPO female both sides
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Ordering Information
FF: Fiber Type CC: Jacket Color
Fiber
Length
Cable OD
Description
Polarity
Packaging
P/N
Count
m
mm
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
5
2.5x5.0
1/Bag
83T FF HA005P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
10
2.5x5.0
1/Bag
83T FF HA010P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
20
2.5x5.0
1/Bag
83T FF HA020P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
30
2.5x5.0
1/Bag
83T FF HA030P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
40
2.5x5.0
1/Bag
83T FF HA040P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
50
2.5x5.0
1/Bag
83T FF HA050P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
60
2.5x5.0
1/Bag
83T FF HA060P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
70
2.5x5.0
1/Bag
83T FF HA070P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
80
2.5x5.0
1/Bag
83T FF HA080P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
90
2.5x5.0
1/Bag
83T FF HA090P-CC 61
MPO Female - MPO Female Plug & Play LS0H Cord
Straight
12
100
2.5x5.0
1/Bag
83T FF HA100P-CC 61
C.5.5.1.1