AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic Multimode and Singlemode Pigtails
Description
This page shows the standard AT&T fiber-optic pigtails made with
multimode or singlemode fibers, terminated with different connectors.
Additional combinations can be selected using the information on page B.3
Buffer type
900µ tight flame retardant LS0H
coating
Strength elements (MTRJ only)
Served aramid and glass yarn
Minicable jacket material (MTRJ only)
Flame retardant LS0H compound
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
Default length
1.5m (other lengths available)
Default jacket colors
Indicated (other colors available)
Ordering Information
Length
Cable OD
Description
Color
Packaging
P/N
m
mm
ST/UPC Multimode OM1 Simplex Pigtail
Blue
1.5
0.9
12/Bag - 60/Box
28PM1A0015T-BL6Q
ST/UPC Multimode OM2 Simplex Pigtail
Orange
1.5
0.9
12/Bag - 60/Box
28PM2A0015T-OR6Q
ST/UPC Multimode OM3 Simplex Pigtail
Turquoise
1.5
0.9
12/Bag - 60/Box
28PM3A0015T-TQ6Q
ST/UPC Multimode OM4 Simplex Pigtail
Purple
1.5
0.9
12/Bag - 60/Box
28PM4A0015T-PU6Q
ST/UPC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2C0015T-YL6Q
FC/UPC Multimode OM1 Simplex Pigtail
Blue
1.5
0.9
12/Bag - 60/Box
28PM1E0015T-BL6Q
FC/UPC Multimode OM2 Simplex Pigtail
Orange
1.5
0.9
12/Bag - 60/Box
28PM2E0015T-OR6Q
FC/UPC Multimode OM3 Simplex Pigtail
Turquoise
1.5
0.9
12/Bag - 60/Box
28PM3E0015T-TQ6Q
FC/UPC Multimode OM4 Simplex Pigtail
Purple
1.5
0.9
12/Bag - 60/Box
28PM4E0015T-PU6Q
FC/UPC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2F0015T-YL6Q
FC/APC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2G0015T-YL6Q
SC/UPC Multimode OM1 Simplex Pigtail
Blue
1.5
0.9
12/Bag - 60/Box
28PM1H0015T-BL6Q
SC/UPC Multimode OM2 Simplex Pigtail
Orange
1.5
0.9
12/Bag - 60/Box
28PM2H0015T-OR6Q
SC/UPC Multimode OM3 Simplex Pigtail
Turquoise
1.5
0.9
12/Bag - 60/Box
28PM3H0015T-TQ6Q
SC/UPC Multimode OM4 Simplex Pigtail
Purple
1.5
0.9
12/Bag - 60/Box
28PM4H0015T-PU6Q
SC/UPC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2J0015T-YL6Q
SC/APC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2K0015T-YL6Q
LSH/UPC Multimode OM1 Simplex Pigtail
Blue
1.5
0.9
12/Bag - 60/Box
28PM1D0015T-BL6Q
LSH/UPC Multimode OM2 Simplex Pigtail
Orange
1.5
0.9
12/Bag - 60/Box
28PM2D0015T-OR6Q
LSH/UPC Multimode OM3 Simplex Pigtail
Turquoise
1.5
0.9
12/Bag - 60/Box
28PM3D0015T-TQ6Q
LSH/UPC Multimode OM4 Simplex Pigtail
Purple
1.5
0.9
12/Bag - 60/Box
28PM4D0015T-PU6Q
LSH/UPC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2L0015T-YL6Q
LSH/APC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2M0015T-YL6Q
LC/UPC Multimode OM1 Simplex Pigtail
Blue
1.5
0.9
12/Bag - 60/Box
28PM1P0015T-BL6Q
LC/UPC Multimode OM2 Simplex Pigtail
Orange
1.5
0.9
12/Bag - 60/Box
28PM2P0015T-OR6Q
LC/UPC Multimode OM3 Simplex Pigtail
Turquoise
1.5
0.9
12/Bag - 60/Box
28PM3P0015T-TQ6Q
LC/UPC Multimode OM4 Simplex Pigtail
Purple
1.5
0.9
12/Bag - 60/Box
28PM4P0015T-PU6Q
LC/UPC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2Q0015T-YL6Q
LC/APC Singlemode OS2 Simplex Pigtail
Yellow
1.5
0.9
12/Bag - 60/Box
28PS2R0015T-YL6Q
MTRJ Male Multimode OM1 Duplex Pigtail
Blue
1.5
1.6x3.2
12/Bag - 60/Box
28PM1S0015T-BL6Q
MTRJ Male Multimode OM2 Duplex Pigtail
Orange
1.5
1.6x3.2
12/Bag - 60/Box
28PM2S0015T-OR6Q
MTRJ Male Multimode OM3 Duplex Pigtail
Turquoise
1.5
1.6x3.2
12/Bag - 60/Box
28PM3S0015T-TQ6Q
MTRJ Male Multimode OM4 Duplex Pigtail
Purple
1.5
1.6x3.2
12/Bag - 60/Box
28PM4S0015T-PU6Q
MTRJ Male Singlemode OS2 Duplex Pigtail
Yellow
1.5
1.6x3.2
12/Bag - 60/Box
28PS2S0015T-YL6Q
B.3.3