AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic ST/UPC Duplex Multimode Zip-Cords
Description
This page shows some of the available combinations of AT&T fiber-optic
Duplex Multimode Zip-Cords made with multimode fibers and terminated
with ST/UPC connectors.
Additional combinations can be selected using the information on page B.3
Fiber type
Select a multimode fiber from page B.6
Buffer type
900µ tight flame retardant LS0H coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
Default jacket colors
MM OM3: Turquoise
MM OM4: Purple
Ordering Information
FF: Fiber Type CC: Jacket Color
Length
Cable OD
Description
Packaging
P/N
m
mm
ST/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
1
3.0x6.0
1/Bag - 12/Box
28D FF AA010T-CC 61
ST/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
2
3.0x6.0
1/Bag - 12/Box
28D FF AA020T-CC 61
ST/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
3
3.0x6.0
1/Bag - 12/Box
28D FF AA030T-CC 61
ST/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
5
3.0x6.0
1/Bag - 12/Box
28D FF AA050T-CC 61
ST/UPC-ST/UPC Duplex Multimode Zip-Cord LS0H
10
3.0x6.0
1/Bag - 12/Box
28D FF AA100T-CC 61
ST/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
1
3.0x6.0
1/Bag - 12/Box
28D FF AE010T-CC 61
ST/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
2
3.0x6.0
1/Bag - 12/Box
28D FF AE020T-CC 61
ST/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
3
3.0x6.0
1/Bag - 12/Box
28D FF AE030T-CC 61
ST/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
5
3.0x6.0
1/Bag - 12/Box
28D FF AE050T-CC 61
ST/UPC-FC/UPC Duplex Multimode Zip-Cord LS0H
10
3.0x6.0
1/Bag - 12/Box
28D FF AE100T-CC 61
ST/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
1
2.0x4.0
1/Bag - 12/Box
28D FF AP010T-CC 61
ST/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
2
2.0x4.0
1/Bag - 12/Box
28D FF AP020T-CC 61
ST/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
3
2.0x4.0
1/Bag - 12/Box
28D FF AP030T-CC 61
ST/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
5
2.0x4.0
1/Bag - 12/Box
28D FF AP050T-CC 61
ST/UPC-LC/UPC Duplex Multimode Zip-Cord LS0H
10
2.0x4.0
1/Bag - 12/Box
28D FF AP100T-CC 61
ST/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
1
2.0x4.0
1/Bag - 12/Box
28D FF AD010T-CC 61
ST/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
2
2.0x4.0
1/Bag - 12/Box
28D FF AD020T-CC 61
ST/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
3
2.0x4.0
1/Bag - 12/Box
28D FF AD030T-CC 61
ST/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
5
2.0x4.0
1/Bag - 12/Box
28D FF AD050T-CC 61
ST/UPC-LSH/UPC Duplex Multimode Zip-Cord LS0H
10
2.0x4.0
1/Bag - 12/Box
28D FF AD100T-CC 61
ST/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF AT010T-CC 61
ST/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF AT020T-CC 61
ST/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF AT030T-CC 61
ST/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF AT050T-CC 61
ST/UPC-MTRJ Female Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF AT100T-CC 61
Examples
ST/UPC-ST/UPC Duplex Zip-Cord LS0H OM1 Orange
1
3.0x6.0
1/Bag - 12/Box
28DM1AA010T-OR61
ST/UPC-MTRJ Female Duplex Zip-Cord LS0H OM3 Turquoise
5
1.6x3.2
1/Bag - 12/Box
28DM3AT050T-TQ61
ST/UPC-LSH/UPC Duplex Zip-Cord LS0H OM4 Purple
10
2.0x4.0
1/Bag - 12/Box
28DM4AD100T-PU61
B.3.2.4.1