AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic LSH Couplers
Description
Fiber Optic Couplers Type LSH (E-2000™)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• EU Directive 2011/65/EU (RoHS-2)
Notes:
a. Each product has a full-length P/N that can be used as ordering information.
b. The default colors are indicated in this pages. Other options available.
c. E-2000 is a trademark of Diamond SA, Switzerland.
Ordering Information
Compatible
Body
Cover
Type
Formation
Sleeve
Packaging
P/N
Fiber
Color
Color
LSH/UPC Coupler
Multimode
Single
Beige
Beige
PB
1/Bag 120/Box
29LM1NV001D-BG61
LSH/UPC Coupler
Singlemode
Single
Blue
Blue
Zirconia
1/Bag 120/Box
29LS1NV001L-BL61
LSH/APC Coupler
Singlemode
Single
Green
Green
Zirconia
1/Bag 120/Box
29LS1NV001M-GN61
LSH/UPC Coupler
Multimode
Double
Beige
Beige
PB
1/Bag 120/Box
29LM1NV002D-BG61
LSH/UPC Coupler
Singlemode
Double
Blue
Blue
Zirconia
1/Bag 120/Box
29LS1NV002L-BL61
LSH/APC Coupler
Singlemode
Double
Green
Green
Zirconia
1/Bag 120/Box
29LS1NV002M-GN61
B.4.1.9