AT&T Cabling Systems
FiberLine
AT&T FiberLine
Outdoor Multi Loose-Tube Jelly-Filled Single-Jacket Optical Fiber Cables
Description
2-288 fibers outdoor all-dielectric multi loose-tube jelly-filled
single-jacket non-armored FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking
Petroleum jelly
Armor
None
Cable jacket material
UV-resistant PE
Fibers and loose-tubes color
TIA-598-C
code
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-40 to +70C
Installation temperature
0 to +50C
Water blocking test
3m cable, 1m water, 24h - IEC
60794-1-2 F5
Default fiber count per tube
Indicated (other options available)
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber FO Outdoor Loose-Tube
2000m
2
1
5
10.5
80
2500
1500
25S FF EN002N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
4-Fiber FO Outdoor Loose-Tube
2000m
4
1
5
10.5
80
2500
1500
25S FF EN004N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
6-Fiber FO Outdoor Loose-Tube
2000m
6
1
5
10.5
80
2500
1500
25S FF EN006N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
8-Fiber FO Outdoor Loose-Tube
2000m
4
2
4
10.5
80
2500
1500
25S FF EN008N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
12-Fiber FO Outdoor Loose-Tube
2000m
4
3
3
10.5
80
2500
1500
25S FF EN012N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
24-Fiber FO Outdoor Loose-Tube
2000m
4
6
0
10.5
80
2500
1500
25S FF EN024N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
36-Fiber FO Outdoor Loose-Tube
2000m
6
6
0
10.5
80
2500
1500
25S FF EN036N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
48-Fiber FO Outdoor Loose-Tube
2000m
8
6
0
11.5
105
2500
1500
25S FF EN048N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
72-Fiber FO Outdoor Loose-Tube
2000m
12
6
0
12.0
115
2500
1500
25S FF EN072N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
96-Fiber FO Outdoor Loose-Tube
2000m
12
8
0
13.5
150
2500
1500
25S FF EN096N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
144-Fiber FO Outdoor Loose-Tube
2000m
12
12
0
17.5
235
2500
1500
25S FF EN144N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
288-Fiber FO Outdoor Loose-Tube
2000m
12
24
0
19.5
320
2500
1500
25S FF EN288N-BK2N
All-Dielectric Jelly-Filled SJ Cable
Drum
B.1.5.1