AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor/Outdoor Multi Loose-Tube Dielectric
Armored Dry-Core Single Jacket Optical Fiber LS0H Cables
Description
2-288 fibers indoor/outdoor all-dielectric multi loose-tube dry-core
single-jacket armored FO cables
Fiber type
Select from FiberLine fiber types
(Section B.6)
Buffer type
PBT jell-filled loose tubes
Central strength member
Rigid all-dielectric FRP
Water blocking elements
Swellable yarn and tapes
Dielectric armor
Swellable glass yarn
Cable jacket material
Flame retardant LS0H UV-resistant
compound
Fibers and tubes color code
TIA-598-C
Jacket color
Black (other colors available)
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-40 to +70C
Installation temperature
0 to +50C
Water blocking test
3m cable, 1m water,
24h - IEC 60794-1-2 F5
Default fiber count per tube
Indicated (other options available)
Ordering Information
FF: Fiber Type
Fibers
Cable
Max. Load N
Tube
Weight
Description
per
Fillers
OD
Packaging
P/N
Short
Long
Count
Kg/Km
Tube
mm
Term
Term
2-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
2
1
5
12.0
123
3000
1500
25R FF AA002N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
4-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
4
1
5
12.0
123
3000
1500
25R FF AA004N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
6-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
6
1
5
12.0
123
3000
1500
25R FF AA006N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
8-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
4
2
4
12.0
123
3000
1500
25R FF AA008N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
12-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
4
3
3
12.0
124
3000
1500
25R FF AA012N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
24-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
6
4
0
12.0
125
3000
1500
25R FF AA024N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
36-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
6
6
0
13.0
146
3000
1500
25R FF AA036N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
48-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
8
6
0
13.0
146
3000
1500
25R FF AA048N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
72-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
12
6
0
13.5
160
3000
1500
25R FF AA072N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
96-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
12
8
0
15.5
195
3000
1500
25R FF AA096N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
144-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
12
12
0
19.0
282
3000
1500
25R FF AA144N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
288-Fiber Indoor/Outdoor LS0H FO Loose-Tube
2000m
12
24
0
21.5
350
3000
1500
25R FF AA288N-BK2N
Dielectric Armored Dry-Core SJ Cable
Drum
B.1.3.3