AT&T Cabling Systems
FiberLine
AT&T FiberLine
Indoor/Outdoor Tight-Buffer Dielectric Armored
Double-Jacket Optical Fiber LS0H Cables (contd.)
Ordering Information - Multi-Unit Cables
FF: Fiber Type
Fiber
Subunit
Cable OD
WeightMax.
Load N
Description
per
Packaging
P/N
Count
mm
Kg/Km
Short
Long
Subunit
Term
Term
18-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
6
3
17.5
275
2500
1500
23R FF AA018M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
24-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
6
4
18.5
295
2500
1500
23R FF AA024M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
36-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
6
6
21.5
395
2500
1500
23R FF AA036M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
48-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
12
4
21.5
395
2500
1500
23R FF AA048M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
60-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
12
5
22.5
425
2500
1500
23R FF AA060M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
72-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
12
6
24.5
510
2500
1500
23R FF AA072M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
96-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
12
8
27.5
625
2500
1500
23R FF AA096M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
144-Fiber LS0H FO Indoor/Outdoor Dielectric
2000m
12
12
33.5
885
2500
1500
23R FF AA144M-BK2N
Armored Dry-Core Tight-Buffer DJ Cable
Drum
B.1.3.1a