AT&T Cabling Systems
CenterLine
AT&T CenterLine Fiber Optic MTP Assemblies
MTP-ST Fiber Optic Harnesses
Description
MTP female to ST/UPC LS0H modular harnesses for plug & play panels
Fiber type
Select a fiber from page B.6.
Cable type
12-fiber tight-buffer round cable
Cable jacket material
Flame retardant LS0H compound
Cable jacket diameter
3.0 mm nom.
Connector types
One MTP female and twelve ST/UPC
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
MM OM3: Turquoise
Default jacket colors
MM OM4: Purple
SM: Yellow
Ordering Information
FF: Fiber Type CC: Jacket Color
Fiber
Length
Cable OD
Description
MTP
ST
Packaging
P/N
Count
m
mm
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
2
3.0
1/Bag
80S FF HA002A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
3
3.0
1/Bag
80S FF HA003A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
5
3.0
1/Bag
80S FF HA005A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
10
3.0
1/Bag
80S FF HA010A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
15
3.0
1/Bag
80S FF HA015A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
20
3.0
1/Bag
80S FF HA020A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
25
3.0
1/Bag
80S FF HA025A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
30
3.0
1/Bag
80S FF HA030A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
40
3.0
1/Bag
80S FF HA040A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
50
3.0
1/Bag
80S FF HA050A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
60
3.0
1/Bag
80S FF HA060A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
70
3.0
1/Bag
80S FF HA070A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
80
3.0
1/Bag
80S FF HA080A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
90
3.0
1/Bag
80S FF HA090A-CC 61
MTP Female to ST/UPC Plug & Play LS0H Harness
1
12
12
100
3.0
1/Bag
80S FF HA100A-CC 61
C.5.4.4