AT&T Cabling Systems
FiberLine
AT&T FiberLine Panels
High-Density MPO Fixed Fiber Optic Panels (contd.)
Ordering Information
Fiber
Fiber
MPO
Size
Description
Polarity
Packaging
P/N
Type
Capacity
Couplers
mm
High-Density MPO to LC/UPC
OS2
72
6
Straight
44.5x483x336
1/Box
27PS2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2
72
6
Flipped
44.5x483x336
1/Box
27ES2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2 BI
72
6
Straight
44.5x483x336
1/Box
27PB2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2 BI
72
6
Flipped
44.5x483x336
1/Box
27EB2HV072P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM1
96
8
Straight
44.5x483x336
1/Box
27PM1HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM1
96
8
Flipped
44.5x483x336
1/Box
27EM1HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM2
96
8
Straight
44.5x483x336
1/Box
27PM2HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM2
96
8
Flipped
44.5x483x336
1/Box
27EM2HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3
96
8
Straight
44.5x483x336
1/Box
27PM3HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3
96
8
Flipped
44.5x483x336
1/Box
27EM3HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3 BI
96
8
Straight
44.5x483x336
1/Box
27PC3HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3 BI
96
8
Flipped
44.5x483x336
1/Box
27EC3HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4
96
8
Straight
44.5x483x336
1/Box
27PM4HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4
96
8
Flipped
44.5x483x336
1/Box
27EM4HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4 BI
96
8
Straight
44.5x483x336
1/Box
27PC4HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4 BI
96
8
Flipped
44.5x483x336
1/Box
27EC4HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2
96
8
Straight
44.5x483x336
1/Box
27PS2HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2
96
8
Flipped
44.5x483x336
1/Box
27ES2HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2 BI
96
8
Straight
44.5x483x336
1/Box
27PB2HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2 BI
96
8
Flipped
44.5x483x336
1/Box
27EB2HV096P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM1
144
12
Straight
44.5x483x336
1/Box
27PM1HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM1
144
12
Flipped
44.5x483x336
1/Box
27EM1HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM2
144
12
Straight
44.5x483x336
1/Box
27PM2HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM2
144
12
Flipped
44.5x483x336
1/Box
27EM2HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3
144
12
Straight
44.5x483x336
1/Box
27PM3HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3
144
12
Flipped
44.5x483x336
1/Box
27EM3HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3 BI
144
12
Straight
44.5x483x336
1/Box
27PC3HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM3 BI
144
12
Flipped
44.5x483x336
1/Box
27EC3HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4
144
12
Straight
44.5x483x336
1/Box
27PM4HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4
144
12
Flipped
44.5x483x336
1/Box
27EM4HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4 BI
144
12
Straight
44.5x483x336
1/Box
27PC4HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OM4 BI
144
12
Flipped
44.5x483x336
1/Box
27EC4HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2
144
12
Straight
44.5x483x336
1/Box
27PS2HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2
144
12
Flipped
44.5x483x336
1/Box
27ES2HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2 BI
144
12
Straight
44.5x483x336
1/Box
27PB2HV144P-BK1U
Fixed Fiber Optic Panel
High-Density MPO to LC/UPC
OS2 BI
144
12
Flipped
44.5x483x336
1/Box
27EB2HV144P-BK1U
Fixed Fiber Optic Panel
BI = Bend-Insensitive
B.2.3.3a