AT&T Cabling Systems
RackLine
AT&T RackLine
Enclosures & Rack Systems Network Cabinets Accessories
Description
Accessories for free standing 19” network cabinets
Cabinet size range
26U, 36U, 42U and 47U
600x800 mm, 600x1000 mm
800x800 mm, 800x1000mm
Standard & EU Directives Conformance
• Mechanical structure conforming to EN 61587-1
• Corrosion resistance (salt spray) acc. to ISO 9227, ASTM B117
• EU Directive 2011/65/EU (RoHS-2)
Ordering Information - Vertical Cable Managements
Applicable
Description
Size
Cabinet Width
Color
P/N
mm
Vertical Cable Management for Server & Network Cabinets with Cover
26U
800
Black
715V080026N-BK51
Vertical Cable Management for Server & Network Cabinets with Cover
36U
800
Black
715V080036N-BK51
Vertical Cable Management for Server & Network Cabinets with Cover
42U
800
Black
715V080042N-BK51
Vertical Cable Management for Server & Network Cabinets with Cover
47U
800
Black
715V080047N-BK51
Ordering Information - Horizontal Cable Managements
Height
Width
Depth
Description
Retainers
Units
Color
Packaging
P/N
mm
mm
mm
Rack-Mount Duct-Type 19” Horizontal Cable Manager
None
1U
44.45
482.60
75.27
Black
1/Box
521NANN075A-BK1U
Rack-Mount Duct-Type 19” Horizontal Cable Manager
Available
1U
44.30
482.00
162.83
Black
1/Box
521NANN162B-BK1U
Rack-Mount Duct-Type 19” Horizontal Cable Manager
Available
2U
88.80
484.84
107.03
Black
1/Box
521NANN107B-BK2U
Rack-Mount Duct-Type 19” Horizontal Cable Manager
Available
2U
88.80
484.74
171.62
Black
1/Box
521NANN171B-BK2U
Rack-Mount Ring-Type 19” Horizontal Cable Manager
None
1U
44.45
482.60
65.00
Black
1/Box
521NANN065C-BK1U
Continued on page D.5.2a
D.5.2