AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic MTRJ Duplex Multimode Zip-Cords
Description
This page shows some of the available combinations of AT&T fiber-optic
Duplex Multimode Zip-Cords made with multimode fibers and terminated
with MTRJ connectors.
Additional combinations can be selected using the information on page B.3
Fiber type
Select a multimode fiber from page B.6
Buffer type
900µ tight flame retardant LS0H coating
Strength elements
Served aramid and glass yarn
Minicable jacket material
Flame retardant LS0H compound
Standard & EU Directives Conformance
• Relevant sections of ANSI/TIA-568-C.3
• Relevant sections of ISO/IEC 11801
• Relevant sections of EN 50173
• Relevant sections of ANSI/TIA/EIA-604 (FOCIS)
• Relevant sections of IEC 60874
• Relevant sections of IEC 61753
• Relevant sections of IEC 61754
• IEC 60332-1 flame test
• IEC 60754 & IEC 61034
• EU Directive 2011/65/EU (RoHS-2)
Mechanical Properties
Short term bend radius
20xOD mm
Long term bend radius
10xOD mm
Operating temperature
-20 to +60C
MM OM1 & OM2: Orange
Default jacket color
MM OM3: Turquoise
MM OM4: Purple
Ordering Information
FF: Fiber Type CC: Jacket Color
Length
Cable OD
Description
Packaging
P/N
m
mm
MTRJ-MTRJ Female Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF TT010T-CC 61
MTRJ-MTRJ Female Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF TT020T-CC 61
MTRJ-MTRJ Female Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF TT030T-CC 61
MTRJ-MTRJ Female Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF TT050T-CC 61
MTRJ-MTRJ Female Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF TT100T-CC 61
MTRJ Female-FC/UPC Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF TE010T-CC 61
MTRJ Female-FC/UPC Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF TE020T-CC 61
MTRJ Female-FC/UPC Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF TE030T-CC 61
MTRJ Female-FC/UPC Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF TE050T-CC 61
MTRJ Female-FC/UPC Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF TE100T-CC 61
MTRJ Female-LC/UPC Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF TP010T-CC 61
MTRJ Female-LC/UPC Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF TP020T-CC 61
MTRJ Female-LC/UPC Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF TP030T-CC 61
MTRJ Female-LC/UPC Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF TP050T-CC 61
MTRJ Female-LC/UPC Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF TP100T-CC 61
MTRJ Female-LSH/UPC Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF TD010T-CC 61
MTRJ Female-LSH/UPC Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF TD020T-CC 61
MTRJ Female-LSH/UPC Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF TD030T-CC 61
MTRJ Female-LSH/UPC Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF TD050T-CC 61
MTRJ Female-LSH/UPC Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF TD100T-CC 61
MTRJ Female-SC/UPC Duplex Multimode Zip-Cord LS0H
1
1.6x3.2
1/Bag - 12/Box
28D FF TH010T-CC 61
MTRJ Female-SC/UPC Duplex Multimode Zip-Cord LS0H
2
1.6x3.2
1/Bag - 12/Box
28D FF TH020T-CC 61
MTRJ Female-SC/UPC Duplex Multimode Zip-Cord LS0H
3
1.6x3.2
1/Bag - 12/Box
28D FF TH030T-CC 61
MTRJ Female-SC/UPC Duplex Multimode Zip-Cord LS0H
5
1.6x3.2
1/Bag - 12/Box
28D FF TH050T-CC 61
MTRJ Female-SC/UPC Duplex Multimode Zip-Cord LS0H
10
1.6x3.2
1/Bag - 12/Box
28D FF TH100T-CC 61
Examples
MTRJ Female-LSH/UPC Duplex Zip-Cord LS0H OM1 Orange
1
2.0x4.0
1/Bag - 12/Box
28DM1TD010T-OR61
MTRJ Female-FC/UPC Duplex Zip-Cord LS0H OM3 Turquoise
5
2.0x4.0
1/Bag - 12/Box
28DM3TE050T-TQ61
MTRJ Female-ST/UPC Duplex Zip-Cord LS0H OM4 Purple
10
2.0x4.0
1/Bag - 12/Box
28DM4TA100T-PU61
B.3.2.6.1