AT&T Cabling Systems
FiberLine
AT&T FiberLine
Fiber Optic Cords and Pigtails
Fiber Optic Cords and Pigtails P/N System
This page shows all the available combinations of AT&T fiber-optic cords and pigtails.
The following steps should be followed to define the exact product needed.
Notes:
a. All AT&T fiber-optic cords and pigtails are halogen-free, low smoke and flame retardant (LS0H).
b. The default cable diameters are indicated in the following sample catalog pages. Other options available.
c. The default formation of all duplex cords is ZIP (FIG-8). Other options available.
The generic P/N of AT&T fiber-optic cords and pigtails has the following format:
28
R
FF
AB
LLL
T
-
CC
61
1. Replace the R with the product type needed.
2. Replace the FF with the relevant Fiber Code selected from page B.6.
3. Replace the A with the relevant Connector Code selected from page B.4.1 for one end of the cord.
4. Replace the B with the relevant Connector Code selected from page B.4.1 for the other end of the cord.
Note: In pigtails B=0.
5. Replace the LLL with the required length in dm.
Examples:
053 = 5.3 m cord length.
185 = 18.5 m cord length.
Note: Default lengths are indicated in the following sample catalog pages.
6. Replace the CC with the required Cable Jacket Color from the table below.
Note: Default colors are indicated in the following sample catalog pages.
Select the Connector Code from section B.4.1, one for each end of the cord.
Indicate the required length in dm.
Example: LLL=053 indicates a length of 5.3 m.
Reserved for options. Default: T.
Select the Cable Jacket Color from the table below.
Default colors indicated in the following
sample catalog pages.
Fiber Optic Cords and Pigtails
28
R
FF
AB
LLL
T
-
CC
61
Select the Fiber Code from page B.6
61 indicates one cord packed in a plastic bag.
Other packaging options available.
C=Simplex LS0H Cord
D=Duplex LS0H Cord
P=LS0H Pigtail
Jacket Colors (CC)
Code
Color
RAL
Code
Color
RAL
Code
Color
RAL
BL
Blue
5015
GY
ATT Gray
9002
BK
Black
9004
OR
Orange
2000
GL
Office Gray
7035
YL
Yellow
1021
GN
Green
6024
WT
White
9003
PU
Purple
4005
BN
Brown
8011
RD
Red
3000
TQ
Turquoise
5018
B.3